[
  {
    "added_include_path": "/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/cores/arduino"
  },
  {
    "added_include_path": "/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx"
  },
  {
    "added_include_path": "/home/arduino/.arduino15/internal/Arduino_RPClite_0.3.0_66fefd6c76c3d010/Arduino_RPClite/src"
  },
  {
    "added_include_path": "/home/arduino/.arduino15/internal/Arduino_RouterBridge_0.4.2_2bacd18211ad070f/Arduino_RouterBridge/src"
  },
  {
    "added_include_path": "/home/arduino/.arduino15/internal/ArxContainer_0.7.0_007f0bb2a1cdefe3/ArxContainer"
  },
  {
    "added_include_path": "/home/arduino/.arduino15/internal/ArxTypeTraits_0.3.2_d65e2aabfeed7838/ArxTypeTraits"
  },
  {
    "added_include_path": "/home/arduino/.arduino15/internal/DebugLog_0.8.4_c199e2cf6415ecc8/DebugLog"
  },
  {
    "added_include_path": "/home/arduino/.arduino15/internal/MsgPack_0.4.2_a0d4adc5044d022c/MsgPack"
  },
  {
    "compile": {
      "source_path": "/home/arduino/ArduinoApps/demo_9_rotary_encoder/.cache/sketch/sketch/sketch.ino.cpp.merged",
      "depfile_path": "/home/arduino/ArduinoApps/demo_9_rotary_encoder/.cache/sketch/sketch/sketch.ino.cpp.merged.libsdetect.d"
    },
    "compile_task": {
      "args": [
        "/home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/arm-zephyr-eabi-g++",
        "-g",
        "-Os",
        "-std=gnu++17",
        "-c",
        "-D_PICOLIBC_CTYPE_SMALL=1",
        "-w",
        "-imacros/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx/llext-edk/include/zephyr/include/generated/zephyr/autoconf.h",
        "-imacros/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx/llext-edk/include/zephyr/include/zephyr/toolchain/zephyr_stdint.h",
        "@/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx/cxxflags.txt",
        "-fno-exceptions",
        "-fno-rtti",
        "-fno-threadsafe-statics",
        "-fno-unwind-tables",
        "-fno-use-cxa-atexit",
        "-lstdc++",
        "-lsupc++",
        "-lnosys",
        "-nostdlib",
        "-lstdc++",
        "-lsupc++",
        "-lm",
        "-fno-exceptions",
        "-fno-rtti",
        "-fdata-sections",
        "-ffunction-sections",
        "-fno-unwind-tables",
        "-mcpu=cortex-m33",
        "-mfloat-abi=hard",
        "-mfpu=fpv5-sp-d16",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DARDUINO=10607",
        "-DARDUINO_UNO_Q",
        "-DARDUINO_ARCH_ZEPHYR",
        "-DARDUINO_ARCH_ZEPHYR",
        "-DARDUINO_LIBRARY_DISCOVERY_PHASE=1",
        "-I/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/cores/arduino",
        "-I/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx",
        "-I/home/arduino/.arduino15/internal/Arduino_RPClite_0.3.0_66fefd6c76c3d010/Arduino_RPClite/src",
        "-I/home/arduino/.arduino15/internal/Arduino_RouterBridge_0.4.2_2bacd18211ad070f/Arduino_RouterBridge/src",
        "-I/home/arduino/.arduino15/internal/ArxContainer_0.7.0_007f0bb2a1cdefe3/ArxContainer",
        "-I/home/arduino/.arduino15/internal/ArxTypeTraits_0.3.2_d65e2aabfeed7838/ArxTypeTraits",
        "-I/home/arduino/.arduino15/internal/DebugLog_0.8.4_c199e2cf6415ecc8/DebugLog",
        "-I/home/arduino/.arduino15/internal/MsgPack_0.4.2_a0d4adc5044d022c/MsgPack",
        "-I/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/cores/arduino/api/deprecated",
        "-I/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/cores/arduino/api/deprecated-avr-comp",
        "-iprefix/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx",
        "@/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx/includes.txt",
        "/home/arduino/ArduinoApps/demo_9_rotary_encoder/.cache/sketch/sketch/sketch.ino.cpp.merged",
        "-o",
        "/dev/null",
        "-MMD",
        "-MF",
        "/home/arduino/ArduinoApps/demo_9_rotary_encoder/.cache/sketch/sketch/sketch.ino.cpp.merged.libsdetect.d"
      ]
    }
  },
  {
    "missing_include_h": ""
  },
  {
    "compile": {
      "source_path": "/home/arduino/.arduino15/internal/Arduino_RouterBridge_0.4.2_2bacd18211ad070f/Arduino_RouterBridge/src/singletons.cpp",
      "depfile_path": "/home/arduino/ArduinoApps/demo_9_rotary_encoder/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.libsdetect.d"
    },
    "compile_task": {
      "args": [
        "/home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/arm-zephyr-eabi-g++",
        "-g",
        "-Os",
        "-std=gnu++17",
        "-c",
        "-D_PICOLIBC_CTYPE_SMALL=1",
        "-w",
        "-imacros/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx/llext-edk/include/zephyr/include/generated/zephyr/autoconf.h",
        "-imacros/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx/llext-edk/include/zephyr/include/zephyr/toolchain/zephyr_stdint.h",
        "@/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx/cxxflags.txt",
        "-fno-exceptions",
        "-fno-rtti",
        "-fno-threadsafe-statics",
        "-fno-unwind-tables",
        "-fno-use-cxa-atexit",
        "-lstdc++",
        "-lsupc++",
        "-lnosys",
        "-nostdlib",
        "-lstdc++",
        "-lsupc++",
        "-lm",
        "-fno-exceptions",
        "-fno-rtti",
        "-fdata-sections",
        "-ffunction-sections",
        "-fno-unwind-tables",
        "-mcpu=cortex-m33",
        "-mfloat-abi=hard",
        "-mfpu=fpv5-sp-d16",
        "-w",
        "-x",
        "c++",
        "-E",
        "-CC",
        "-DARDUINO=10607",
        "-DARDUINO_UNO_Q",
        "-DARDUINO_ARCH_ZEPHYR",
        "-DARDUINO_ARCH_ZEPHYR",
        "-DARDUINO_LIBRARY_DISCOVERY_PHASE=1",
        "-I/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/cores/arduino",
        "-I/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx",
        "-I/home/arduino/.arduino15/internal/Arduino_RPClite_0.3.0_66fefd6c76c3d010/Arduino_RPClite/src",
        "-I/home/arduino/.arduino15/internal/Arduino_RouterBridge_0.4.2_2bacd18211ad070f/Arduino_RouterBridge/src",
        "-I/home/arduino/.arduino15/internal/ArxContainer_0.7.0_007f0bb2a1cdefe3/ArxContainer",
        "-I/home/arduino/.arduino15/internal/ArxTypeTraits_0.3.2_d65e2aabfeed7838/ArxTypeTraits",
        "-I/home/arduino/.arduino15/internal/DebugLog_0.8.4_c199e2cf6415ecc8/DebugLog",
        "-I/home/arduino/.arduino15/internal/MsgPack_0.4.2_a0d4adc5044d022c/MsgPack",
        "-I/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/cores/arduino/api/deprecated",
        "-I/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/cores/arduino/api/deprecated-avr-comp",
        "-iprefix/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx",
        "@/home/arduino/.arduino15/packages/arduino/hardware/zephyr/0.55.0/variants/arduino_uno_q_stm32u585xx/includes.txt",
        "/home/arduino/.arduino15/internal/Arduino_RouterBridge_0.4.2_2bacd18211ad070f/Arduino_RouterBridge/src/singletons.cpp",
        "-o",
        "/dev/null",
        "-MMD",
        "-MF",
        "/home/arduino/ArduinoApps/demo_9_rotary_encoder/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.libsdetect.d"
      ]
    }
  },
  {
    "missing_include_h": ""
  }
]