Archive member included to satisfy reference by file (symbol)

/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o (arduino::Print::println(char const*))
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o (arduino::Stream::setTimeout(unsigned long))
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o (arduino::String::String(arduino::String&&))
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o) (dtostrf)
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o (memcpy)
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
                              (main)
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o (operator new(unsigned int))
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o) (start_static_threads())
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o (pinMode)
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o (Serial2)
/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o) (map(long, long, long, long, long))
/home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
                              /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o (std::__throw_bad_alloc())

Discarded input sections

 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text.__tcf_0  0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeEv
                0x0000000000000000       0x16 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker5clearEv
                0x0000000000000000       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker13getRawBytePtrEjj
                0x0000000000000000       0x1e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN8RpcErrorC2Ev
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8UnpackerC2Ev
                0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt12_Vector_baseIhSaIhEED2Ev
                0x0000000000000000       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text.__tcf_2  0x0000000000000000       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text.__tcf_1  0x0000000000000000       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt6vectorIhSaIhEE14_M_move_assignEOS1_St17integral_constantIbLb1EE.isra.0
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIhEET_jj
                0x0000000000000000       0x1e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker7getTypeEj
                0x0000000000000000       0x58 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker7getTypeEv
                0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11unpackInt32Ev
                0x0000000000000000       0x58 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11unpackInt64Ev
                0x0000000000000000       0x60 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker9unpackNilEv
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker7isArrayEv
                0x0000000000000000       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker5isMapEv
                0x0000000000000000       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11unpackInt16Ev
                0x0000000000000000       0x4c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker13unpackFloat32Ev
                0x0000000000000000       0x60 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker13unpackFloat64Ev
                0x0000000000000000       0x6c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker10unpackInt5Ev
                0x0000000000000000       0x4c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11unpackUInt7Ev
                0x0000000000000000       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11unpackUInt8Ev
                0x0000000000000000       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesItEET_jj
                0x0000000000000000       0x26 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker12unpackUInt16Ev
                0x0000000000000000       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIjEET_jj
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker14getElementSizeEj
                0x0000000000000000      0x11c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker15unpackArraySizeEv
                0x0000000000000000       0x78 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker12unpackUInt32Ev
                0x0000000000000000       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker13unpackMapSizeEv
                0x0000000000000000       0x78 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIyEET_jj
                0x0000000000000000       0x3a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker12unpackUInt64Ev
                0x0000000000000000       0x4c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIaEET_jj
                0x0000000000000000       0x1e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker10unpackInt8Ev
                0x0000000000000000       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker13isTimestamp32Ev
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker13isTimestamp64Ev
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker13isTimestamp96Ev
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIcEET_jj
                0x0000000000000000       0x1e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_4type9ArraySizeEJEEEbRT_DpOT0_
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_6object5nil_tEJEEEbRT_DpOT0_
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeIbJEEEbRT_DpOT0_
                0x0000000000000000       0x68 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS_6StringEJEEEbRT_DpOT0_
                0x0000000000000000      0x174 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_6object8timespecEJEEEbRT_DpOT0_
                0x0000000000000000       0xc4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt12_Vector_baseIjSaIjEED2Ev
                0x0000000000000000       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RPCRequestILj256EED2Ev
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt6vectorIjSaIjEE17_M_realloc_insertIJRjEEEvN9__gnu_cxx17__normal_iteratorIPjS1_EEDpOT_
                0x0000000000000000       0xdc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker4feedEPKhj
                0x0000000000000000       0x78 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7RpcCallIJEE8setErrorEiN7arduino6StringE
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNKSt6vectorIhSaIhEE12_M_check_lenEjPKc
                0x0000000000000000       0x38 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeISt6vectorIhSaIhEEJEEEbRT_DpOT0_
                0x0000000000000000      0x13c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer9packUInt8Eh
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer15packRawReversedIjEEvRKT_
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer10packUInt32Ej
                0x0000000000000000       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer15packRawReversedItEEvRKT_
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer13packArraySizeEj
                0x0000000000000000       0x58 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer10packUInt16Et
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer12packRawBytesEPKcj
                0x0000000000000000       0x9c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer4packERKNS_6StringE
                0x0000000000000000       0x7c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker9unpackIntIiEENSt9enable_ifIXaaaaaaaasrSt13is_arithmeticIT_E5valuesrSt11is_integralIS5_E5valuentsrSt7is_sameIS5_bE5valuentsrS9_INSt9remove_cvIS5_E4typeEPcE5valuesrSt9is_signedIS5_E5valueES5_E4typeEv
                0x0000000000000000       0xd0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeIiJEEEbRT_DpOT0_
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11unpackFloatIfEENSt9enable_ifIXaasrSt13is_arithmeticIT_E5valuesrSt17is_floating_pointIS5_E5valueES5_E4typeEv
                0x0000000000000000      0x118 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11unpackFloatIdEENSt9enable_ifIXaasrSt13is_arithmeticIT_E5valuesrSt17is_floating_pointIS5_E5valueES5_E4typeEv
                0x0000000000000000      0x118 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_4type9ArraySizeEJRiEEEbRT_DpOT0_
                0x0000000000000000       0x44 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNK10RpcDecoderILj1024EE4sendEPKhj
                0x0000000000000000       0x22 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN9RPCClient8send_rpcIJRKjEEEbRKN7arduino6StringERjDpOT_.isra.0
                0x0000000000000000       0x84 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RpcDecoderILj1024EE7consumeEjj
                0x0000000000000000       0x50 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RpcDecoderILj1024EE7discardEv
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeI8RpcErrorJRNS0_6object5nil_tEEEEbRT_DpOT0_
                0x0000000000000000       0x90 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker10unpackUIntIjEENSt9enable_ifIXaaaaaaaasrSt13is_arithmeticIT_E5valuesrSt11is_integralIS5_E5valuentsrSt7is_sameIS5_bE5valuentsrS9_INSt9remove_cvIS5_E4typeEPcE5valuentsrSt9is_signedIS5_E5valueES5_E4typeEv
                0x0000000000000000       0x80 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeIjJRNS_6StringEEEEbRT_DpOT0_
                0x0000000000000000       0x44 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RpcDecoderILj1024EE16fetch_rpc_methodEv
                0x0000000000000000       0xe8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RPCRequestILj256EE22unpack_request_headersEv
                0x0000000000000000       0xb8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN9RPCServer15process_requestILj256EEEvR10RPCRequestIXT_EE
                0x0000000000000000      0x138 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_4type9ArraySizeEJRiRjEEEbRT_DpOT0_
                0x0000000000000000       0x78 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RpcDecoderILj1024EE12get_responseIN7arduino7msgpack6object5nil_tEEEbjRT_R8RpcError
                0x0000000000000000      0x17c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RpcDecoderILj1024EE12get_responseIbEEbjRT_R8RpcError
                0x0000000000000000      0x17c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt11__copy_moveILb0ELb1ESt26random_access_iterator_tagE8__copy_mIhEEPT_PKS3_S6_S4_
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt11__copy_moveILb1ELb1ESt26random_access_iterator_tagE8__copy_mIhEEPT_PKS3_S6_S4_
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .rodata._ZN7arduino7msgpack6object3extC2EaPKhj.str1.1
                0x0000000000000000       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6object3extC2EaPKhj
                0x0000000000000000      0x104 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker9unpackExtEv
                0x0000000000000000      0x178 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerE
                0x0000000000000000      0x27c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RpcDecoderILj1024EE12parse_packetEv
                0x0000000000000000      0x13c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RpcDecoderILj1024EE6decodeEv
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN9RPCServer7get_rpcILj256EEEbR10RPCRequestIXT_EEN7arduino6StringE
                0x0000000000000000       0xd0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .rodata._ZN11BridgeClass11update_safeEv.str1.1
                0x0000000000000000        0x9 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN11BridgeClass11update_safeEv
                0x0000000000000000       0xf4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._Z10__loopHookv
                0x0000000000000000       0x44 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN9RPCClient12get_responseIN7arduino7msgpack6object5nil_tEEEbjRT_R8RpcError
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN8RpcUtils6detail9unpackMapERN7arduino7msgpack8UnpackerERj
                0x0000000000000000       0x80 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7RpcCallIJRjEE8setErrorEiN7arduino6StringE
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7RpcCallIJRjEE7isErrorEv
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7RpcCallIJRjEED2Ev
                0x0000000000000000      0x118 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN10RpcDecoderILj1024EE12get_responseISt6vectorIhSaIhEEEEbjRT_R8RpcError
                0x0000000000000000      0x17c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7RpcCallIJRjEE6resultISt6vectorIhSaIhEEEEbRT_
                0x0000000000000000      0x134 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .rodata._ZN13BridgeMonitorILj512EE5_readEj.str1.1
                0x0000000000000000        0x9 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN13BridgeMonitorILj512EE5_readEj
                0x0000000000000000      0x120 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZGVN12RouterBridge3HCIE
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZGVZN7arduino7msgpack8Unpacker10from_arrayIJRiRNS_6StringEEEEbDpOT_E2sz
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN7arduino7msgpack8Unpacker10from_arrayIJRiRNS_6StringEEEEbDpOT_E2sz
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZN12RouterBridge3HCIE
                0x0000000000000000       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE1t
                0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZGVZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE1e
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE1e
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE6map_sz
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE6arr_sz
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZGVZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE5bytes
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE5bytes
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZGVZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE6string
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE6string
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE5num64
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE5num32
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE7integer
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE1b
                0x0000000000000000        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE3nil
                0x0000000000000000        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .text.analogReference
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .debug_info    0x0000000000000000     0x15b3 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .debug_abbrev  0x0000000000000000      0x31c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .debug_loclists
                0x0000000000000000       0x23 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .debug_aranges
                0x0000000000000000       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .debug_rnglists
                0x0000000000000000       0x13 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .debug_line    0x0000000000000000      0x3c3 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .debug_str     0x0000000000000000     0x1738 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .debug_frame   0x0000000000000000       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print17availableForWriteEv
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5flushEv
                0x0000000000000000        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5writeEPKhj
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEPKNS_19__FlashStringHelperE
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printERKNS_6StringE
                0x0000000000000000        0xa /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEPKc
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEc
                0x0000000000000000        0x6 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printERKNS_9PrintableE
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnERKNS_6StringE
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEc
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnERKNS_9PrintableE
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print11printNumberEmh
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEli
                0x0000000000000000       0x50 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEii
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEii
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEli
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEmi
                0x0000000000000000       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEhi
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEhi
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEji
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEji
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEmi
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print14printULLNumberEyh
                0x0000000000000000       0xfc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printExi
                0x0000000000000000       0x5c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnExi
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEyi
                0x0000000000000000       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEyi
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .rodata._ZN7arduino5Print10printFloatEdi.str1.1
                0x0000000000000000        0xe /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print10printFloatEdi
                0x0000000000000000      0x1b4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print5printEdi
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text._ZN7arduino5Print7printlnEdi
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .rodata._ZTVN7arduino5PrintE
                0x0000000000000000       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream9timedPeekEv
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream13peekNextDigitENS_13LookaheadModeEb
                0x0000000000000000       0x58 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream8parseIntENS_13LookaheadModeEc
                0x0000000000000000       0x70 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream10parseFloatENS_13LookaheadModeEc
                0x0000000000000000      0x138 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream14readBytesUntilEcPcj
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .rodata._ZN7arduino6Stream10readStringEv.str1.1
                0x0000000000000000        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream10readStringEv
                0x0000000000000000       0x38 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream15readStringUntilEc
                0x0000000000000000       0x44 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream9findMultiEPNS0_11MultiTargetEi
                0x0000000000000000       0xa8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream9findUntilEPKcjS2_j
                0x0000000000000000       0x50 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream9findUntilEPKcS2_
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream4findEPKcj
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text._ZN7arduino6Stream4findEPKc
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2EPKcj
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String4copyEPKNS_19__FlashStringHelperEj
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2Ec
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2Ehh
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2Eih
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2Ejh
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2Elh
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2Emh
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2Efh
                0x0000000000000000       0x4c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2Edh
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringaSEPKNS_19__FlashStringHelperE
                0x0000000000000000       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringC2EPKNS_19__FlashStringHelperE
                0x0000000000000000       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatERKS0_
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEPKc.part.0
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEPKc
                0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEh
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEi
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEj
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEl
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEm
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEf
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEd
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6concatEPKNS_19__FlashStringHelperE
                0x0000000000000000       0x44 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperERKNS_6StringE
                0x0000000000000000       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEPKc
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEc
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEh
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEi
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEj
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEl
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEm
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEf
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEd
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduinoplERKNS_15StringSumHelperEPKNS_19__FlashStringHelperE
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String9compareToEPKc
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String16equalsIgnoreCaseERKS0_
                0x0000000000000000       0x38 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String10startsWithERKS0_j
                0x0000000000000000       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String10startsWithERKS0_
                0x0000000000000000       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String8endsWithERKS0_
                0x0000000000000000       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String9setCharAtEjc
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6StringixEj
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6StringixEj
                0x0000000000000000       0x12 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String6charAtEj
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String8getBytesEPhjj
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String7indexOfEcj
                0x0000000000000000       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String7indexOfEc
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String7indexOfERKS0_j
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String7indexOfERKS0_
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String11lastIndexOfEcj
                0x0000000000000000       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String11lastIndexOfEc
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String11lastIndexOfERKS0_j
                0x0000000000000000       0x54 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String11lastIndexOfERKS0_
                0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .rodata._ZNK7arduino6String9substringEjj.str1.1
                0x0000000000000000        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String9substringEjj
                0x0000000000000000       0x4c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String7replaceEcc
                0x0000000000000000       0x16 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String7replaceERKS0_S2_
                0x0000000000000000      0x12c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6removeEjj
                0x0000000000000000       0x38 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String6removeEj
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String11toLowerCaseEv
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String11toUpperCaseEv
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZN7arduino6String4trimEv
                0x0000000000000000       0x58 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String5toIntEv
                0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String8toDoubleEv
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text._ZNK7arduino6String7toFloatEv
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .bss._ZZN7arduino6StringixEjE19dummy_writable_char
                0x0000000000000000        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .rodata._ZN7arduino6String22DBL_MAX_DECIMAL_PLACESE
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .rodata._ZN7arduino6String22FLT_MAX_DECIMAL_PLACESE
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .rodata.dtostrf.str1.1
                0x0000000000000000        0x9 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .text.dtostrf  0x0000000000000000       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .text.ltoa     0x0000000000000000       0x80 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .text.itoa     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .text.ultoa    0x0000000000000000       0x64 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .text.utoa     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .debug_info    0x0000000000000000      0x3de /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .debug_abbrev  0x0000000000000000      0x128 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .debug_loclists
                0x0000000000000000      0x3e1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .debug_aranges
                0x0000000000000000       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .debug_rnglists
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .debug_line    0x0000000000000000      0x32d /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .debug_str     0x0000000000000000      0x37a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .debug_frame   0x0000000000000000       0xa0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(itoa.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strnlen  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strchr   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strrchr  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strstr   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strncmp  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strcasecmp
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strncpy  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strcat   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strcpy   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.memcmp   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strtok   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.memchr   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strdup   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.memmem   0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strtod   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strtol   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.strtoul  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.atoi     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.atof     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.atol     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.calloc   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.rand     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.srand    0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.isspace  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.isalnum  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.tolower  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.toupper  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.isalpha  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.iscntrl  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.isdigit  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.isgraph  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.isprint  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.isupper  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.islower  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.isxdigit
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.acos     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.asin     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.atan     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.atan2    0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.cos      0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.exp      0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.exp2     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.fmod     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.ldexp    0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.log10    0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.log2     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.log      0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.pow      0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.sin      0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.sqrt     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.tan      0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.acosf    0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.asinf    0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.atanf    0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.atan2f   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.cosf     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.logf     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.sinf     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.sqrtf    0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.tanf     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.__aeabi_dadd
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.__aeabi_dcmpgt
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.puts     0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.putchar  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.vsnprintf
                0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text.exit     0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text._exit    0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .text._Z10__loopHookv
                0x0000000000000000        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .entry_point   0x0000000000000000       0xb8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._Znaj    0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZnwjSt11align_val_t
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZnajSt11align_val_t
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZnwjSt11align_val_tSt9nothrow_t
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZnajSt11align_val_tRKSt9nothrow_t
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZnwjSt9nothrow_t
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZnajRKSt9nothrow_t
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZnajPv  0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZdlPv   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZdaPv   0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZdaPvj  0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZdlPvRKSt9nothrow_t
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZdaPvRKSt9nothrow_t
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZdlPvS_
                0x0000000000000000        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._ZdaPvS_
                0x0000000000000000        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .rodata._ZSt7nothrow
                0x0000000000000000        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.gpio_pin_get_dt
                0x0000000000000000       0x2a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._ZN12_GLOBAL__N_123find_gpio_port_callbackEPK6device
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._ZN12_GLOBAL__N_118handleGpioCallbackEPK6deviceP13gpio_callbackj
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._ZN12_GLOBAL__N_119setInterruptHandlerEhPFvvE.part.0
                0x0000000000000000       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._ZL14find_pin_timerhb
                0x0000000000000000       0x88 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.k_mutex_unlock.constprop.0.isra.0
                0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z14tone_expiry_cbP7k_timer
                0x0000000000000000       0x74 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z22digitalPinToPortDeviceh
                0x0000000000000000       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z20digitalPinToPinIndexh
                0x0000000000000000       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.digitalRead
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z4tonehjm
                0x0000000000000000      0x188 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z6noToneh
                0x0000000000000000       0x88 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.micros   0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z21analogWriteResolutioni
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z21analogWriteResolutionv
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.analogWrite
                0x0000000000000000      0x144 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z11analogWrite7dacPinsi
                0x0000000000000000       0xb4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.analogReference
                0x0000000000000000        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z20analogReadResolutioni
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z20analogReadResolutionv
                0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.analogRead
                0x0000000000000000       0xd4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z10randomSeedm
                0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z6randomll
                0x0000000000000000       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z6randoml
                0x0000000000000000       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.pulseIn  0x0000000000000000       0xd4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.enableInterrupt
                0x0000000000000000       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.attachInterrupt
                0x0000000000000000       0xb8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.disableInterrupt
                0x0000000000000000       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.detachInterrupt
                0x0000000000000000       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z10interruptsv
                0x0000000000000000       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z12noInterruptsv
                0x0000000000000000       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text._Z21digitalPinToInterrupth
                0x0000000000000000       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .rodata.CSWTCH.164
                0x0000000000000000       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .data._ZL15read_resolution
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .data._ZL24_analog_write_resolution
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 ._k_mutex.static.timer_cfg_lock_
                0x0000000000000000       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .bss._ZN12_GLOBAL__N_1L19interrupts_disabledE
                0x0000000000000000        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .bss._ZN12_GLOBAL__N_1L7irq_keyE
                0x0000000000000000        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .bss._ZN12_GLOBAL__N_1L23dac_channel_initializedE
                0x0000000000000000        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .rodata._ZN12_GLOBAL__N_1L10dac_ch_cfgE
                0x0000000000000000        0x6 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .rodata._ZN12_GLOBAL__N_1L11arduino_adcE
                0x0000000000000000       0x60 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .rodata._ZN12_GLOBAL__N_1L16arduino_pwm_pinsE
                0x0000000000000000       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .rodata._ZN12_GLOBAL__N_1L11arduino_pwmE
                0x0000000000000000      0x100 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .bss._ZN12_GLOBAL__N_113port_callbackE
                0x0000000000000000      0x534 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .group         0x0000000000000000        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .group         0x0000000000000000        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .text._Z12serial1Eventv
                0x0000000000000000        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .text._Z12serial2Eventv
                0x0000000000000000        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .text._ZN7arduino14serialEventRunEv
                0x0000000000000000       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .data          0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .bss           0x0000000000000000        0x0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .text._Z3maplllll
                0x0000000000000000       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .text._Z8makeWordt
                0x0000000000000000        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .text._Z8makeWordhh
                0x0000000000000000        0x6 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .debug_info    0x0000000000000000      0x168 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .debug_abbrev  0x0000000000000000       0xc1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .debug_loclists
                0x0000000000000000       0x51 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .debug_aranges
                0x0000000000000000       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .debug_rnglists
                0x0000000000000000       0x1f /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .debug_line    0x0000000000000000      0x1b6 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .debug_str     0x0000000000000000      0x370 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .comment       0x0000000000000000       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .debug_frame   0x0000000000000000       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .ARM.attributes
                0x0000000000000000       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Common.cpp.o)
 .text          0x0000000000000000        0x0 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .data          0x0000000000000000        0x0 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .bss           0x0000000000000000        0x0 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt21__throw_bad_exceptionv
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt28__throw_bad_array_new_lengthv
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt16__throw_bad_castv
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt18__throw_bad_typeidv
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt19__throw_logic_errorPKc
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt20__throw_domain_errorPKc
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt24__throw_invalid_argumentPKc
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt20__throw_out_of_rangePKc
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt24__throw_out_of_range_fmtPKcz
                0x0000000000000000        0x8 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt21__throw_runtime_errorPKc
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt19__throw_range_errorPKc
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt22__throw_overflow_errorPKc
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .text.unlikely._ZSt23__throw_underflow_errorPKc
                0x0000000000000000        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
 .ARM.attributes
                0x0000000000000000       0x38 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)

Memory Configuration

Name             Origin             Length             Attributes
*default*        0x0000000000000000 0xffffffffffffffff

Linker script and memory map

LOAD /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a
LOAD /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libsupc++_nano.a
LOAD /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libnosys.a
LOAD /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
LOAD /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
LOAD /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/analogReference.cpp.o
START GROUP
LOAD /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a
LOAD /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a
LOAD /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libsupc++_nano.a
LOAD /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libm_nano.a
END GROUP

.rodata         0x0000000000000000      0x2ac
 *(.rodata._ZL12arduino_pins)
 .rodata._ZL12arduino_pins
                0x0000000000000000      0x230 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 *(.rodata._ZTV13BridgeMonitorILj512EE)
 .rodata._ZTV13BridgeMonitorILj512EE
                0x0000000000000230       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000000230                vtable for BridgeMonitor<512u>
 *(.rodata._ZTV15SerialTransport)
 .rodata._ZTV15SerialTransport
                0x0000000000000254       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000254                vtable for SerialTransport
 *(.rodata._ZTVN7arduino12ZephyrSerialE)
 .rodata._ZTVN7arduino12ZephyrSerialE
                0x0000000000000274       0x38 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000000274                vtable for arduino::ZephyrSerial

.llext.rodata.noreloc
                0x00000000000002ac      0x391
 *(.rodata._ZL12stepSequence)
 .rodata._ZL12stepSequence
                0x00000000000002ac       0x80 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata._ZN10RpcDecoderILj1024EE12get_responseIN7arduino7msgpack6object5nil_tEEEbjRT_R8RpcError.str1.1)
 .rodata._ZN10RpcDecoderILj1024EE12get_responseIN7arduino7msgpack6object5nil_tEEEbjRT_R8RpcError.str1.1
                0x000000000000032c       0x7b /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 *(.rodata._ZN10RpcDecoderILj1024EE12get_responseIbEEbjRT_R8RpcError.str1.1)
 .rodata._ZN10RpcDecoderILj1024EE12get_responseIbEEbjRT_R8RpcError.str1.1
                0x00000000000003a7       0x7b /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata._ZN11BridgeClass11update_safeEv.str1.1)
 .rodata._ZN11BridgeClass11update_safeEv.str1.1
                0x0000000000000422        0x9 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata._ZN11BridgeClass5beginEm.str1.1)
 .rodata._ZN11BridgeClass5beginEm.str1.1
                0x000000000000042b       0x45 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata._ZN13BridgeMonitorILj512EE5_readEj.str1.1)
 .rodata._ZN13BridgeMonitorILj512EE5_readEj.str1.1
                0x0000000000000470       0x17 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata._ZN13BridgeMonitorILj512EE5writeEPKhj.str1.1)
 .rodata._ZN13BridgeMonitorILj512EE5writeEPKhj.str1.1
                0x0000000000000487        0xa /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 *(.rodata._ZN13BridgeMonitorILj512EEcvbEv.str1.1)
 .rodata._ZN13BridgeMonitorILj512EEcvbEv.str1.1
                0x0000000000000491       0x4d /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 *(.rodata._ZN7RpcCallIJEE6resultIbEEbRT_.part.0.str1.1)
 .rodata._ZN7RpcCallIJEE6resultIbEEbRT_.part.0.str1.1
                0x00000000000004de       0x21 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata._ZN7RpcCallIJEEC2ERKN7arduino6StringEP9RPCClientP7k_mutexS8_.str1.1)
 .rodata._ZN7RpcCallIJEEC2ERKN7arduino6StringEP9RPCClientP7k_mutexS8_.str1.1
                0x00000000000004ff       0x1e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata._ZN7arduino5Print7printlnEv.str1.1)
 .rodata._ZN7arduino5Print7printlnEv.str1.1
                0x000000000000051d        0x3 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 *(.rodata._ZN7arduino7msgpack6object3extC2EaPKhj.str1.1)
 .rodata._ZN7arduino7msgpack6object3extC2EaPKhj.str1.1
                0x0000000000000520       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata._ZN8RpcErrorC2Ev.str1.1)
 .rodata._ZN8RpcErrorC2Ev.str1.1
                0x0000000000000548        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .rodata._ZN8RpcErrorC2Ev.str1.1
                0x0000000000000549        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 *(.rodata._ZNSt6vectorIjSaIjEE17_M_realloc_insertIJRjEEEvN9__gnu_cxx17__normal_iteratorIPjS1_EEDpOT_.str1.1)
 .rodata._ZNSt6vectorIjSaIjEE17_M_realloc_insertIJRjEEEvN9__gnu_cxx17__normal_iteratorIPjS1_EEDpOT_.str1.1
                0x000000000000054a       0x1a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .rodata._ZNSt6vectorIjSaIjEE17_M_realloc_insertIJRjEEEvN9__gnu_cxx17__normal_iteratorIPjS1_EEDpOT_.str1.1
                0x0000000000000564       0x1a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 *(.rodata.loop.str1.1)
 .rodata.loop.str1.1
                0x000000000000057e       0x1f /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata.setup.str1.1)
 .rodata.setup.str1.1
                0x000000000000059d       0x4f /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 *(.rodata.str1.1)
 .rodata.str1.1
                0x00000000000005ec       0x51 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)

.rel.rodata
 *(.rel.rodata)
 *(.rel.rodata.*)

.rela.rodata
 *(.rela.rodata)
 *(.rela.rodata.*)

/DISCARD/
 *(.ARM.attributes)
 *(.ARM.attributes.*)
 *(.ARM.exidx)
 *(.ARM.exidx.*)
 *(.ARM.extidx)
 *(.ARM.extidx.*)
 *(.ARM.extab)
 *(.ARM.extab.*)
 *(.comment)
 *(.comment.*)
 *(.llvmbc)
 *(.llvmcmd)
 *(.eh_frame)
 *stdexcept.o()
 *eh_*.o()
 *cow-stdexcept.o()
 *cow-string-inst.o()

.text           0x0000000000000000     0x57ac
 *(.text)
 *(.stub)
 *(.text*)
 .text._ZN15SerialTransport9availableEv
                0x0000000000000000       0x12 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000000                SerialTransport::available()
 .text._ZN15SerialTransport5writeEPKhj
                0x0000000000000012       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000012                SerialTransport::write(unsigned char const*, unsigned int)
 .text._ZN15SerialTransportD2Ev
                0x0000000000000022        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000022                SerialTransport::~SerialTransport()
                0x0000000000000022                SerialTransport::~SerialTransport()
 .text.k_yield  0x0000000000000024        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text.k_mutex_lock
                0x000000000000002c        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text.__tcf_0  0x0000000000000034       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN15SerialTransportD0Ev
                0x0000000000000044       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000044                SerialTransport::~SerialTransport()
 .text._ZN15SerialTransport4readEPhj
                0x0000000000000058       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000058                SerialTransport::read(unsigned char*, unsigned int)
 .text._ZN15SerialTransport9read_byteERh
                0x0000000000000080       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000080                SerialTransport::read_byte(unsigned char&)
 .text._ZSt14__relocate_a_1IhhENSt9enable_ifIXsrSt24__is_bitwise_relocatableIT_vE5valueEPS2_E4typeES4_S4_S4_RSaIT0_E.isra.0
                0x00000000000000a0       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZNSt12_Vector_baseIhSaIhEE11_M_allocateEj.isra.0
                0x00000000000000c0       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text.k_mutex_unlock.isra.0
                0x00000000000000e0        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text.k_mutex_init.isra.0
                0x00000000000000e8        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text.k_msleep.constprop.0.isra.0
                0x00000000000000f0        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeEv
                0x00000000000000fc       0x16 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000000fc                arduino::msgpack::Unpacker::deserialize()
 .text._ZN7arduino7msgpack8Unpacker5clearEv
                0x0000000000000112       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000112                arduino::msgpack::Unpacker::clear()
 .text._ZNK7arduino7msgpack8Unpacker13getRawBytePtrEjj
                0x0000000000000126       0x1e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000126                arduino::msgpack::Unpacker::getRawBytePtr(unsigned int, unsigned int) const
 .text._ZN8RpcErrorC2Ev
                0x0000000000000144       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000144                RpcError::RpcError()
                0x0000000000000144                RpcError::RpcError()
 .text._ZN17RpcDecoderManager10getDecoderER10ITransport
                0x0000000000000170       0x7c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000170                RpcDecoderManager::getDecoder(ITransport&)
 .text._ZN17RpcDecoderManager11getInstanceEv
                0x00000000000001ec       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000001ec                RpcDecoderManager::getInstance()
 .text._ZN7arduino7msgpack8UnpackerC2Ev
                0x000000000000021c       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000021c                arduino::msgpack::Unpacker::Unpacker()
                0x000000000000021c                arduino::msgpack::Unpacker::Unpacker()
 .text._ZN10RPCRequestILj256EEC2Ev
                0x000000000000022c       0x4c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000022c                RPCRequest<256u>::RPCRequest()
                0x000000000000022c                RPCRequest<256u>::RPCRequest()
 .text._ZN11BridgeClass10is_startedEv
                0x0000000000000278       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000278                BridgeClass::is_started()
 .text._Z7setStepiiii
                0x00000000000002a4       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000002a4                setStep(int, int, int, int)
 .text._Z9stopMotorv
                0x00000000000002d4       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000002d4                stopMotor()
 .text._Z6rotateibi
                0x00000000000002ec       0x68 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000002ec                rotate(int, bool, int)
 .text._ZNSt12_Vector_baseIhSaIhEED2Ev
                0x0000000000000354       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000354                std::_Vector_base<unsigned char, std::allocator<unsigned char> >::~_Vector_base()
                0x0000000000000354                std::_Vector_base<unsigned char, std::allocator<unsigned char> >::~_Vector_base()
 .text.__tcf_2  0x000000000000036c       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text.__tcf_1  0x0000000000000380       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZNSt6vectorIhSaIhEE14_M_move_assignEOS1_St17integral_constantIbLb1EE.isra.0
                0x0000000000000394       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIhEET_jj
                0x00000000000003c8       0x1e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000003c8                unsigned char arduino::msgpack::Unpacker::getRawBytes<unsigned char>(unsigned int, unsigned int) const
 *fill*         0x00000000000003e6        0x2 
 .text._ZNK7arduino7msgpack8Unpacker7getTypeEj
                0x00000000000003e8       0x58 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000003e8                arduino::msgpack::Unpacker::getType(unsigned int) const
 .text._ZNK7arduino7msgpack8Unpacker7getTypeEv
                0x0000000000000440       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000440                arduino::msgpack::Unpacker::getType() const
 .text._ZN7arduino7msgpack8Unpacker11unpackInt32Ev
                0x0000000000000450       0x58 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000450                arduino::msgpack::Unpacker::unpackInt32()
 .text._ZN7arduino7msgpack8Unpacker11unpackInt64Ev
                0x00000000000004a8       0x60 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000004a8                arduino::msgpack::Unpacker::unpackInt64()
 .text._ZN7arduino7msgpack8Unpacker9unpackNilEv
                0x0000000000000508       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000508                arduino::msgpack::Unpacker::unpackNil()
 .text._ZNK7arduino7msgpack8Unpacker7isArrayEv
                0x0000000000000544       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000544                arduino::msgpack::Unpacker::isArray() const
 .text._ZNK7arduino7msgpack8Unpacker5isMapEv
                0x0000000000000564       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000564                arduino::msgpack::Unpacker::isMap() const
 .text._ZN7arduino7msgpack8Unpacker11unpackInt16Ev
                0x0000000000000584       0x4c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000584                arduino::msgpack::Unpacker::unpackInt16()
 .text._ZN7arduino7msgpack8Unpacker13unpackFloat32Ev
                0x00000000000005d0       0x60 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000005d0                arduino::msgpack::Unpacker::unpackFloat32()
 .text._ZN7arduino7msgpack8Unpacker13unpackFloat64Ev
                0x0000000000000630       0x6c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000630                arduino::msgpack::Unpacker::unpackFloat64()
 .text._ZN7arduino7msgpack8Unpacker10unpackInt5Ev
                0x000000000000069c       0x4c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000069c                arduino::msgpack::Unpacker::unpackInt5()
 .text._ZN7arduino7msgpack8Unpacker11unpackUInt7Ev
                0x00000000000006e8       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000006e8                arduino::msgpack::Unpacker::unpackUInt7()
 .text._ZN7arduino7msgpack8Unpacker11unpackUInt8Ev
                0x0000000000000730       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000730                arduino::msgpack::Unpacker::unpackUInt8()
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesItEET_jj
                0x0000000000000778       0x26 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000778                unsigned short arduino::msgpack::Unpacker::getRawBytes<unsigned short>(unsigned int, unsigned int) const
 *fill*         0x000000000000079e        0x2 
 .text._ZN7arduino7msgpack8Unpacker12unpackUInt16Ev
                0x00000000000007a0       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000007a0                arduino::msgpack::Unpacker::unpackUInt16()
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIjEET_jj
                0x00000000000007e8       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000007e8                unsigned int arduino::msgpack::Unpacker::getRawBytes<unsigned int>(unsigned int, unsigned int) const
 .text._ZNK7arduino7msgpack8Unpacker14getElementSizeEj
                0x000000000000081c      0x11c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000081c                arduino::msgpack::Unpacker::getElementSize(unsigned int) const
 .text._ZN7arduino7msgpack8Unpacker15unpackArraySizeEv
                0x0000000000000938       0x78 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000938                arduino::msgpack::Unpacker::unpackArraySize()
 .text._ZN7arduino7msgpack8Unpacker12unpackUInt32Ev
                0x00000000000009b0       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000009b0                arduino::msgpack::Unpacker::unpackUInt32()
 .text._ZN7arduino7msgpack8Unpacker13unpackMapSizeEv
                0x00000000000009f8       0x78 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000009f8                arduino::msgpack::Unpacker::unpackMapSize()
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIyEET_jj
                0x0000000000000a70       0x3a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000a70                unsigned long long arduino::msgpack::Unpacker::getRawBytes<unsigned long long>(unsigned int, unsigned int) const
 *fill*         0x0000000000000aaa        0x2 
 .text._ZN7arduino7msgpack8Unpacker12unpackUInt64Ev
                0x0000000000000aac       0x4c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000aac                arduino::msgpack::Unpacker::unpackUInt64()
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIaEET_jj
                0x0000000000000af8       0x1e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000af8                signed char arduino::msgpack::Unpacker::getRawBytes<signed char>(unsigned int, unsigned int) const
 *fill*         0x0000000000000b16        0x2 
 .text._ZN7arduino7msgpack8Unpacker10unpackInt8Ev
                0x0000000000000b18       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000b18                arduino::msgpack::Unpacker::unpackInt8()
 .text._ZNK7arduino7msgpack8Unpacker13isTimestamp32Ev
                0x0000000000000b60       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000b60                arduino::msgpack::Unpacker::isTimestamp32() const
 .text._ZNK7arduino7msgpack8Unpacker13isTimestamp64Ev
                0x0000000000000b8c       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000b8c                arduino::msgpack::Unpacker::isTimestamp64() const
 .text._ZNK7arduino7msgpack8Unpacker13isTimestamp96Ev
                0x0000000000000bb8       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000bb8                arduino::msgpack::Unpacker::isTimestamp96() const
 .text._ZNK7arduino7msgpack8Unpacker11getRawBytesIcEET_jj
                0x0000000000000bf8       0x1e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000bf8                char arduino::msgpack::Unpacker::getRawBytes<char>(unsigned int, unsigned int) const
 *fill*         0x0000000000000c16        0x2 
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_4type9ArraySizeEJEEEbRT_DpOT0_
                0x0000000000000c18       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000c18                bool arduino::msgpack::Unpacker::deserialize<arduino::msgpack::type::ArraySize>(arduino::msgpack::type::ArraySize&)
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_6object5nil_tEJEEEbRT_DpOT0_
                0x0000000000000c58       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000c58                bool arduino::msgpack::Unpacker::deserialize<arduino::msgpack::object::nil_t>(arduino::msgpack::object::nil_t&)
 .text._ZN7arduino7msgpack8Unpacker11deserializeIbJEEEbRT_DpOT0_
                0x0000000000000c98       0x68 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000c98                bool arduino::msgpack::Unpacker::deserialize<bool>(bool&)
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS_6StringEJEEEbRT_DpOT0_
                0x0000000000000d00      0x174 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000d00                bool arduino::msgpack::Unpacker::deserialize<arduino::String>(arduino::String&)
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_6object8timespecEJEEEbRT_DpOT0_
                0x0000000000000e74       0xc4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000e74                bool arduino::msgpack::Unpacker::deserialize<arduino::msgpack::object::timespec>(arduino::msgpack::object::timespec&)
 .text._ZNSt12_Vector_baseIjSaIjEED2Ev
                0x0000000000000f38       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000f38                std::_Vector_base<unsigned int, std::allocator<unsigned int> >::~_Vector_base()
                0x0000000000000f38                std::_Vector_base<unsigned int, std::allocator<unsigned int> >::~_Vector_base()
 .text._ZN10RPCRequestILj256EED2Ev
                0x0000000000000f50       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000f50                RPCRequest<256u>::~RPCRequest()
                0x0000000000000f50                RPCRequest<256u>::~RPCRequest()
 .text._ZNSt6vectorIjSaIjEE17_M_realloc_insertIJRjEEEvN9__gnu_cxx17__normal_iteratorIPjS1_EEDpOT_
                0x0000000000000f7c       0xdc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000000f7c                void std::vector<unsigned int, std::allocator<unsigned int> >::_M_realloc_insert<unsigned int&>(__gnu_cxx::__normal_iterator<unsigned int*, std::vector<unsigned int, std::allocator<unsigned int> > >, unsigned int&)
 .text._ZN7arduino7msgpack8Unpacker4feedEPKhj
                0x0000000000001058       0x78 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001058                arduino::msgpack::Unpacker::feed(unsigned char const*, unsigned int)
 .text._ZN7RpcCallIJEE8setErrorEiN7arduino6StringE
                0x00000000000010d0       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000010d0                RpcCall<>::setError(int, arduino::String)
 .text._ZN7RpcCallIJEEC2ERKN7arduino6StringEP9RPCClientP7k_mutexS8_
                0x0000000000001110       0x7c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001110                RpcCall<>::RpcCall(arduino::String const&, RPCClient*, k_mutex*, k_mutex*)
                0x0000000000001110                RpcCall<>::RpcCall(arduino::String const&, RPCClient*, k_mutex*, k_mutex*)
 .text._ZN7RpcCallIJEE6resultIbEEbRT_.part.0
                0x000000000000118c       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN7RpcCallIJEE7isErrorEv
                0x00000000000011c0       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000011c0                RpcCall<>::isError()
 .text._ZNKSt6vectorIhSaIhEE12_M_check_lenEjPKc
                0x00000000000011f4       0x38 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000011f4                std::vector<unsigned char, std::allocator<unsigned char> >::_M_check_len(unsigned int, char const*) const
 .text._ZNSt6vectorIhSaIhEE12emplace_backIJRKhEEERhDpOT_.isra.0
                0x000000000000122c       0x90 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZNSt6vectorIhSaIhEE12emplace_backIJhEEERhDpOT_.isra.0
                0x00000000000012bc       0x90 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeISt6vectorIhSaIhEEJEEEbRT_DpOT0_
                0x000000000000134c      0x13c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000134c                bool arduino::msgpack::Unpacker::deserialize<std::vector<unsigned char, std::allocator<unsigned char> >>(std::vector<unsigned char, std::allocator<unsigned char> >&)
 .text._ZN7arduino7msgpack6Packer11packRawByteERKNS0_4TypeE.isra.0
                0x0000000000001488       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN7arduino7msgpack6Packer9packUInt8Eh
                0x00000000000014a0       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000014a0                arduino::msgpack::Packer::packUInt8(unsigned char)
 .text._ZNSt6vectorIhSaIhEE12emplace_backIJRhEEES3_DpOT_.isra.0
                0x00000000000014cc       0x90 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN7arduino7msgpack6Packer15packRawReversedIjEEvRKT_
                0x000000000000155c       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000155c                void arduino::msgpack::Packer::packRawReversed<unsigned int>(unsigned int const&)
 .text._ZN7arduino7msgpack6Packer10packUInt32Ej
                0x0000000000001578       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001578                arduino::msgpack::Packer::packUInt32(unsigned int)
 .text._ZN7arduino7msgpack6Packer15packRawReversedItEEvRKT_
                0x00000000000015a0       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000015a0                void arduino::msgpack::Packer::packRawReversed<unsigned short>(unsigned short const&)
 .text._ZN7arduino7msgpack6Packer13packArraySizeEj
                0x00000000000015bc       0x58 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000015bc                arduino::msgpack::Packer::packArraySize(unsigned int)
 .text._ZN7arduino7msgpack6Packer10packUInt16Et
                0x0000000000001614       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001614                arduino::msgpack::Packer::packUInt16(unsigned short)
 .text._ZN7arduino7msgpack6Packer11packIntegerIjEENSt9enable_ifIXaaaaaasrSt13is_arithmeticIT_E5valuesrSt11is_integralIS5_E5valuentsrSt7is_sameIS5_bE5valuentsrS9_INSt9remove_cvIS5_E4typeEPcE5valueEvE4typeERKS5_.isra.0
                0x0000000000001640       0x50 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN7arduino7msgpack6Packer11packIntegerIiEENSt9enable_ifIXaaaaaasrSt13is_arithmeticIT_E5valuesrSt11is_integralIS5_E5valuentsrSt7is_sameIS5_bE5valuentsrS9_INSt9remove_cvIS5_E4typeEPcE5valueEvE4typeERKS5_.isra.0
                0x0000000000001690       0xb8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN7arduino7msgpack6Packer12packRawBytesEPKcj
                0x0000000000001748       0x9c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001748                arduino::msgpack::Packer::packRawBytes(char const*, unsigned int)
 .text._ZN7arduino7msgpack6Packer4packERKNS_6StringE
                0x00000000000017e4       0x7c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000017e4                arduino::msgpack::Packer::pack(arduino::String const&)
 .text._ZN7arduino7msgpack8Unpacker9unpackIntIiEENSt9enable_ifIXaaaaaaaasrSt13is_arithmeticIT_E5valuesrSt11is_integralIS5_E5valuentsrSt7is_sameIS5_bE5valuentsrS9_INSt9remove_cvIS5_E4typeEPcE5valuesrSt9is_signedIS5_E5valueES5_E4typeEv
                0x0000000000001860       0xd0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001860                std::enable_if<(((std::is_arithmetic<int>::value&&std::is_integral<int>::value)&&(!std::is_same<int, bool>::value))&&(!std::is_same<std::remove_cv<int>::type, char*>::value))&&std::is_signed<int>::value, int>::type arduino::msgpack::Unpacker::unpackInt<int>()
 .text._ZN7arduino7msgpack8Unpacker11deserializeIiJEEEbRT_DpOT0_
                0x0000000000001930       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001930                bool arduino::msgpack::Unpacker::deserialize<int>(int&)
 .text._ZN7arduino7msgpack8Unpacker11unpackFloatIfEENSt9enable_ifIXaasrSt13is_arithmeticIT_E5valuesrSt17is_floating_pointIS5_E5valueES5_E4typeEv
                0x0000000000001970      0x118 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001970                std::enable_if<std::is_arithmetic<float>::value&&std::is_floating_point<float>::value, float>::type arduino::msgpack::Unpacker::unpackFloat<float>()
 .text._ZN7arduino7msgpack8Unpacker11unpackFloatIdEENSt9enable_ifIXaasrSt13is_arithmeticIT_E5valuesrSt17is_floating_pointIS5_E5valueES5_E4typeEv
                0x0000000000001a88      0x118 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001a88                std::enable_if<std::is_arithmetic<double>::value&&std::is_floating_point<double>::value, double>::type arduino::msgpack::Unpacker::unpackFloat<double>()
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_4type9ArraySizeEJRiEEEbRT_DpOT0_
                0x0000000000001ba0       0x44 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001ba0                bool arduino::msgpack::Unpacker::deserialize<arduino::msgpack::type::ArraySize, int&>(arduino::msgpack::type::ArraySize&, int&)
 .text._ZNK10RpcDecoderILj1024EE4sendEPKhj
                0x0000000000001be4       0x22 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001be4                RpcDecoder<1024u>::send(unsigned char const*, unsigned int) const
 *fill*         0x0000000000001c06        0x2 
 .text._ZN9RPCClient8send_rpcIJEEEbRKN7arduino6StringERjDpOT_.isra.0
                0x0000000000001c08       0x8c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN9RPCClient8send_rpcIJRKjEEEbRKN7arduino6StringERjDpOT_.isra.0
                0x0000000000001c94       0x94 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN11BridgeClass6notifyIJiEEEvN7arduino6StringEDpOT_
                0x0000000000001d28       0xac /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001d28                void BridgeClass::notify<int>(arduino::String, int&&)
 .text._ZNK9RPCServer13send_responseILj256EEEbRK10RPCRequestIXT_EE.isra.0
                0x0000000000001dd4       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN10RpcDecoderILj1024EE7consumeEjj
                0x0000000000001df8       0x50 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001df8                RpcDecoder<1024u>::consume(unsigned int, unsigned int)
 .text._ZN10RpcDecoderILj1024EE7discardEv
                0x0000000000001e48       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001e48                RpcDecoder<1024u>::discard()
 .text._ZN7arduino7msgpack8Unpacker11deserializeI8RpcErrorJRNS0_6object5nil_tEEEEbRT_DpOT0_
                0x0000000000001e74       0x90 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001e74                bool arduino::msgpack::Unpacker::deserialize<RpcError, arduino::msgpack::object::nil_t&>(RpcError&, arduino::msgpack::object::nil_t&)
 .text._ZN7RpcCallIJRjEE8setErrorEiN7arduino6StringE
                0x0000000000001f04       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001f04                RpcCall<unsigned int&>::setError(int, arduino::String)
 .text._ZN7RpcCallIJRjEE7isErrorEv
                0x0000000000001f44       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001f44                RpcCall<unsigned int&>::isError()
 .text._ZN7arduino7msgpack8Unpacker10unpackUIntIjEENSt9enable_ifIXaaaaaaaasrSt13is_arithmeticIT_E5valuesrSt11is_integralIS5_E5valuentsrSt7is_sameIS5_bE5valuentsrS9_INSt9remove_cvIS5_E4typeEPcE5valuentsrSt9is_signedIS5_E5valueES5_E4typeEv
                0x0000000000001f78       0x80 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001f78                std::enable_if<(((std::is_arithmetic<unsigned int>::value&&std::is_integral<unsigned int>::value)&&(!std::is_same<unsigned int, bool>::value))&&(!std::is_same<std::remove_cv<unsigned int>::type, char*>::value))&&(!std::is_signed<unsigned int>::value), unsigned int>::type arduino::msgpack::Unpacker::unpackUInt<unsigned int>()
 .text._ZN7arduino7msgpack8Unpacker11deserializeIjJRNS_6StringEEEEbRT_DpOT0_
                0x0000000000001ff8       0x44 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000001ff8                bool arduino::msgpack::Unpacker::deserialize<unsigned int, arduino::String&>(unsigned int&, arduino::String&)
 .text._ZN10RpcDecoderILj1024EE16fetch_rpc_methodEv
                0x000000000000203c       0xe8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000203c                RpcDecoder<1024u>::fetch_rpc_method()
 .text._ZN10RPCRequestILj256EE22unpack_request_headersEv
                0x0000000000002124       0xb8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000002124                RPCRequest<256u>::unpack_request_headers()
 .text._ZN9RPCServer15process_requestILj256EEEvR10RPCRequestIXT_EE
                0x00000000000021dc      0x138 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000021dc                void RPCServer::process_request<256u>(RPCRequest<256u>&)
 .text._ZN7arduino7msgpack8Unpacker11deserializeINS0_4type9ArraySizeEJRiRjEEEbRT_DpOT0_
                0x0000000000002314       0xa0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000002314                bool arduino::msgpack::Unpacker::deserialize<arduino::msgpack::type::ArraySize, int&, unsigned int&>(arduino::msgpack::type::ArraySize&, int&, unsigned int&)
 .text._ZN10RpcDecoderILj1024EE12get_responseIbEEbjRT_R8RpcError
                0x00000000000023b4      0x17c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000023b4                bool RpcDecoder<1024u>::get_response<bool>(unsigned int, bool&, RpcError&)
 .text._ZN10RpcDecoderILj1024EE12get_responseIN7arduino6StringEEEbjRT_R8RpcError
                0x0000000000002530      0x17c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000002530                bool RpcDecoder<1024u>::get_response<arduino::String>(unsigned int, arduino::String&, RpcError&)
 .text._ZN10RpcDecoderILj1024EE12get_responseIN7arduino7msgpack6object5nil_tEEEbjRT_R8RpcError
                0x00000000000026ac      0x17c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000026ac                bool RpcDecoder<1024u>::get_response<arduino::msgpack::object::nil_t>(unsigned int, arduino::msgpack::object::nil_t&, RpcError&)
 .text._ZN10RpcDecoderILj1024EE12get_responseISt6vectorIhSaIhEEEEbjRT_R8RpcError
                0x0000000000002828      0x17c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000002828                bool RpcDecoder<1024u>::get_response<std::vector<unsigned char, std::allocator<unsigned char> > >(unsigned int, std::vector<unsigned char, std::allocator<unsigned char> >&, RpcError&)
 .text._ZNSt11__copy_moveILb0ELb1ESt26random_access_iterator_tagE8__copy_mIhEEPT_PKS3_S6_S4_
                0x00000000000029a4       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000029a4                unsigned char* std::__copy_move<false, true, std::random_access_iterator_tag>::__copy_m<unsigned char>(unsigned char const*, unsigned char const*, unsigned char*)
 .text._ZNSt11__copy_moveILb1ELb1ESt26random_access_iterator_tagE8__copy_mIhEEPT_PKS3_S6_S4_
                0x00000000000029c0       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000029c0                unsigned char* std::__copy_move<true, true, std::random_access_iterator_tag>::__copy_m<unsigned char>(unsigned char const*, unsigned char const*, unsigned char*)
 .text._ZN7arduino7msgpack6object3extC2EaPKhj
                0x00000000000029dc      0x104 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000029dc                arduino::msgpack::object::ext::ext(signed char, unsigned char const*, unsigned int)
                0x00000000000029dc                arduino::msgpack::object::ext::ext(signed char, unsigned char const*, unsigned int)
 .text._ZN7arduino7msgpack8Unpacker9unpackExtEv
                0x0000000000002ae0      0x178 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000002ae0                arduino::msgpack::Unpacker::unpackExt()
 .text._ZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerE
                0x0000000000002c58      0x27c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000002c58                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)
 .text._ZN10RpcDecoderILj1024EE12parse_packetEv
                0x0000000000002ed4      0x13c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000002ed4                RpcDecoder<1024u>::parse_packet()
 .text._ZN10RpcDecoderILj1024EE6decodeEv
                0x0000000000003010       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003010                RpcDecoder<1024u>::decode()
 .text._ZN9RPCServer7get_rpcILj256EEEbR10RPCRequestIXT_EEN7arduino6StringE
                0x0000000000003050       0xd0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003050                bool RPCServer::get_rpc<256u>(RPCRequest<256u>&, arduino::String)
 .text._ZN11BridgeClass11update_safeEv
                0x0000000000003120       0xb0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003120                BridgeClass::update_safe()
 .text._Z10__loopHookv
                0x00000000000031d0       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000031d0                __loopHook()
 .text._ZN11BridgeClass6updateEv
                0x00000000000031f8       0xb0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000031f8                BridgeClass::update()
 .text._Z16updateEntryPointPvS_S_
                0x00000000000032a8       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000032a8                updateEntryPoint(void*, void*, void*)
 .text._ZN7RpcCallIJEE6resultIbEEbRT_
                0x00000000000032d0      0x114 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000032d0                bool RpcCall<>::result<bool>(bool&)
 .text._ZN9RPCClient12get_responseIN7arduino7msgpack6object5nil_tEEEbjRT_R8RpcError
                0x00000000000033e4       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000033e4                bool RPCClient::get_response<arduino::msgpack::object::nil_t>(unsigned int, arduino::msgpack::object::nil_t&, RpcError&)
 .text._ZN7RpcCallIJRjEED2Ev
                0x0000000000003424      0x118 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003424                RpcCall<unsigned int&>::~RpcCall()
                0x0000000000003424                RpcCall<unsigned int&>::~RpcCall()
 .text._ZN7RpcCallIJEED2Ev
                0x000000000000353c       0xfc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000353c                RpcCall<>::~RpcCall()
                0x000000000000353c                RpcCall<>::~RpcCall()
 .text._ZN11BridgeClass5beginEm
                0x0000000000003638      0x1f0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003638                BridgeClass::begin(unsigned long)
 .text._ZN7RpcCallIJRjEE6resultISt6vectorIhSaIhEEEEbRT_
                0x0000000000003828      0x134 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003828                bool RpcCall<unsigned int&>::result<std::vector<unsigned char, std::allocator<unsigned char> > >(std::vector<unsigned char, std::allocator<unsigned char> >&)
 .text._ZN13BridgeMonitorILj512EE5_readEj
                0x000000000000395c      0x188 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000395c                BridgeMonitor<512u>::_read(unsigned int)
 .text.loop     0x0000000000003ae4      0x100 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003ae4                loop
 .text._ZN7RpcCallIJEE6resultIN7arduino6StringEEEbRT_
                0x0000000000003be4      0x114 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003be4                bool RpcCall<>::result<arduino::String>(arduino::String&)
 .text.setup    0x0000000000003cf8      0x168 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003cf8                setup
 .text._ZN8RpcUtils6detail9unpackMapERN7arduino7msgpack8UnpackerERj
                0x0000000000003e60       0x80 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000003e60                RpcUtils::detail::unpackMap(arduino::msgpack::Unpacker&, unsigned int&)
 .text._GLOBAL__sub_I_setup
                0x0000000000003ee0       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._GLOBAL__sub_D_setup
                0x0000000000003f0c       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .text._ZN7arduino5Print17availableForWriteEv
                0x0000000000003f2c        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000003f2c                arduino::Print::availableForWrite()
 .text._ZN7arduino5Print5flushEv
                0x0000000000003f30        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000003f30                arduino::Print::flush()
 .text._ZN13BridgeMonitorILj512EE5writeEh
                0x0000000000003f32       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000003f32                BridgeMonitor<512u>::write(unsigned char)
 *fill*         0x0000000000003f4a        0x2 
 .text.k_yield  0x0000000000003f4c        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text.k_mutex_lock
                0x0000000000003f54        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZSt14__relocate_a_1IhhENSt9enable_ifIXsrSt24__is_bitwise_relocatableIT_vE5valueEPS2_E4typeES4_S4_S4_RSaIT0_E.isra.0
                0x0000000000003f5c       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt12_Vector_baseIhSaIhEE11_M_allocateEj.isra.0
                0x0000000000003f7c       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text.k_mutex_unlock.isra.0
                0x0000000000003f9c        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7RpcCallIJEE7isErrorEv.isra.0
                0x0000000000003fa4       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7RpcCallIJRN7arduino6StringEEE7isErrorEv.isra.0
                0x0000000000003fcc       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN13BridgeMonitorILj512EE4readEv
                0x0000000000003ff4       0x68 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000003ff4                BridgeMonitor<512u>::read()
 .text._ZN13BridgeMonitorILj512EE4peekEv
                0x000000000000405c       0x44 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x000000000000405c                BridgeMonitor<512u>::peek()
 .text.k_msleep.constprop.0.isra.0
                0x00000000000040a0        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt6vectorIhSaIhEE12emplace_backIJRKhEEERhDpOT_.isra.0
                0x00000000000040ac       0x90 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt6vectorIhSaIhEE12emplace_backIJhEEERhDpOT_.isra.0
                0x000000000000413c       0x90 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer11packRawByteERKNS0_4TypeE.isra.0
                0x00000000000041cc       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZNSt6vectorIhSaIhEE12emplace_backIJRhEEES3_DpOT_.isra.0
                0x00000000000041e4       0x90 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer11packIntegerIjEENSt9enable_ifIXaaaaaasrSt13is_arithmeticIT_E5valuesrSt11is_integralIS5_E5valuentsrSt7is_sameIS5_bE5valuentsrS9_INSt9remove_cvIS5_E4typeEPcE5valueEvE4typeERKS5_.isra.0
                0x0000000000004274       0x50 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer11packIntegerIiEENSt9enable_ifIXaaaaaasrSt13is_arithmeticIT_E5valuesrSt11is_integralIS5_E5valuentsrSt7is_sameIS5_bE5valuentsrS9_INSt9remove_cvIS5_E4typeEPcE5valueEvE4typeERKS5_.isra.0
                0x00000000000042c4       0xb8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack6Packer9serializeIJRKiRjRKNS_6StringEEEEvRKNS0_4type9ArraySizeEDpOT_.isra.0
                0x000000000000437c       0x38 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN9RPCClient8send_rpcIJEEEbRKN7arduino6StringERjDpOT_.isra.0
                0x00000000000043b4       0x74 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN9RPCClient8send_rpcIJRKN7arduino6StringEEEEbS4_RjDpOT_.isra.0
                0x0000000000004428       0x84 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino7msgpack8Unpacker11deserializeIjJEEEbRT_DpOT0_
                0x00000000000044ac       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x00000000000044ac                bool arduino::msgpack::Unpacker::deserialize<unsigned int>(unsigned int&)
 .text._ZN13BridgeMonitorILj512EEcvbEv
                0x00000000000044ec      0x28c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x00000000000044ec                BridgeMonitor<512u>::operator bool()
 .text._ZN11BridgeClass6notifyIJRN7arduino6StringEEEEvS2_DpOT_
                0x0000000000004778       0xac /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000004778                void BridgeClass::notify<arduino::String&>(arduino::String, arduino::String&)
 .text._ZN7RpcCallIJRN7arduino6StringEEE8setErrorEiS1_
                0x0000000000004824       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000004824                RpcCall<arduino::String&>::setError(int, arduino::String)
 .text._ZN7RpcCallIJRN7arduino6StringEEED2Ev
                0x0000000000004864      0x118 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000004864                RpcCall<arduino::String&>::~RpcCall()
                0x0000000000004864                RpcCall<arduino::String&>::~RpcCall()
 .text._ZN10RpcDecoderILj1024EE12get_responseIjEEbjRT_R8RpcError
                0x000000000000497c      0x17c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x000000000000497c                bool RpcDecoder<1024u>::get_response<unsigned int>(unsigned int, unsigned int&, RpcError&)
 .text._ZN13BridgeMonitorILj512EE5writeEPKhj
                0x0000000000004af8      0x1fc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000004af8                BridgeMonitor<512u>::write(unsigned char const*, unsigned int)
 .text._ZN13BridgeMonitorILj512EE9availableEv
                0x0000000000004cf4       0x44 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000004cf4                BridgeMonitor<512u>::available()
 .text._GLOBAL__sub_I_Bridge
                0x0000000000004d38       0xc0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._GLOBAL__sub_D_Bridge
                0x0000000000004df8       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .text._ZN7arduino5Print5writeEPKc
                0x0000000000004e18       0x24 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
                0x0000000000004e18                arduino::Print::write(char const*)
 .text._ZN7arduino5Print7printlnEv
                0x0000000000004e3c       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
                0x0000000000004e3c                arduino::Print::println()
 .text._ZN7arduino5Print7printlnEPKNS_19__FlashStringHelperE
                0x0000000000004e50       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
                0x0000000000004e50                arduino::Print::println(arduino::__FlashStringHelper const*)
 .text._ZN7arduino5Print7printlnEPKc
                0x0000000000004e6c        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
                0x0000000000004e6c                arduino::Print::println(char const*)
 .text._ZN7arduino6Stream9timedReadEv
                0x0000000000004e74       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
                0x0000000000004e74                arduino::Stream::timedRead()
 .text._ZN7arduino6Stream10setTimeoutEm
                0x0000000000004ea0        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
                0x0000000000004ea0                arduino::Stream::setTimeout(unsigned long)
 .text._ZN7arduino6Stream9readBytesEPcj
                0x0000000000004ea4       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
                0x0000000000004ea4                arduino::Stream::readBytes(char*, unsigned int)
 .text._ZN7arduino6StringC2EOS0_
                0x0000000000004ed0       0x16 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000004ed0                arduino::String::String(arduino::String&&)
                0x0000000000004ed0                arduino::String::String(arduino::String&&)
 *fill*         0x0000000000004ee6        0x2 
 .text._ZN7arduino6StringD2Ev
                0x0000000000004ee8       0x14 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000004ee8                arduino::String::~String()
                0x0000000000004ee8                arduino::String::~String()
 .text._ZN7arduino6String10invalidateEv
                0x0000000000004efc       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000004efc                arduino::String::invalidate()
 .text._ZN7arduino6String12changeBufferEj
                0x0000000000004f18       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000004f18                arduino::String::changeBuffer(unsigned int)
 .text._ZN7arduino6String7reserveEj
                0x0000000000004f34       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000004f34                arduino::String::reserve(unsigned int)
 .text._ZN7arduino6String4copyEPKcj
                0x0000000000004f5c       0x3c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000004f5c                arduino::String::copy(char const*, unsigned int)
 .text._ZN7arduino6StringC2EPKc
                0x0000000000004f98       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000004f98                arduino::String::String(char const*)
                0x0000000000004f98                arduino::String::String(char const*)
 .text._ZN7arduino6String4moveERS0_
                0x0000000000004fc4       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000004fc4                arduino::String::move(arduino::String&)
 .text._ZN7arduino6StringaSERKS0_
                0x0000000000004ff0       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000004ff0                arduino::String::operator=(arduino::String const&)
 .text._ZN7arduino6StringC2ERKS0_
                0x0000000000005018       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000005018                arduino::String::String(arduino::String const&)
                0x0000000000005018                arduino::String::String(arduino::String const&)
 .text._ZN7arduino6StringaSEOS0_
                0x0000000000005030       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000005030                arduino::String::operator=(arduino::String&&)
 .text._ZN7arduino6StringaSEPKc
                0x0000000000005040       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000005040                arduino::String::operator=(char const*)
 .text._ZN7arduino6String6concatEPKcj
                0x0000000000005070       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x0000000000005070                arduino::String::concat(char const*, unsigned int)
 .text._ZN7arduino6String6concatEc
                0x00000000000050b0       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x00000000000050b0                arduino::String::concat(char)
 .text._ZNK7arduino6String9compareToERKS0_
                0x00000000000050cc       0x30 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x00000000000050cc                arduino::String::compareTo(arduino::String const&) const
 .text._ZNK7arduino6String6equalsERKS0_
                0x00000000000050fc       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x00000000000050fc                arduino::String::equals(arduino::String const&) const
 .text._ZNK7arduino6String6equalsEPKc
                0x000000000000511c       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
                0x000000000000511c                arduino::String::equals(char const*) const
 .text.memcpy   0x0000000000005144        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x0000000000005144                memcpy
 .text.memmove  0x000000000000514c        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x000000000000514c                memmove
 .text.strlen   0x0000000000005154        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x0000000000005154                strlen
 .text.strcmp   0x000000000000515c        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x000000000000515c                strcmp
 .text.memset   0x0000000000005164        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x0000000000005164                memset
 .text.malloc   0x000000000000516c        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x000000000000516c                malloc
 .text.realloc  0x0000000000005174        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x0000000000005174                realloc
 .text.free     0x000000000000517c        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x000000000000517c                free
 .text.atexit   0x0000000000005184        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x0000000000005184                atexit
 .text.abort    0x000000000000518c        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
                0x000000000000518c                abort
 .text.initVariant
                0x0000000000005198        0x2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
                0x0000000000005198                initVariant
 *fill*         0x000000000000519a        0x2 
 .text.main     0x000000000000519c       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
                0x000000000000519c                main
 .text._ZL10new_helperj
                0x00000000000051c8       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .text._Znwj    0x00000000000051d8        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
                0x00000000000051d8                operator new(unsigned int)
 .text._ZnwjPv  0x00000000000051e0        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
                0x00000000000051e0                operator new(unsigned int, void*)
 .text._ZdlPvj  0x00000000000051e4        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
                0x00000000000051e4                operator delete(void*, unsigned int)
 .text._Z20start_static_threadsv
                0x00000000000051ec       0x6c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
                0x00000000000051ec                start_static_threads()
 .text.gpio_pin_set_dt.isra.0
                0x0000000000005258       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.gpio_pin_configure_dt.isra.0
                0x0000000000005280       0x2a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 *fill*         0x00000000000052aa        0x2 
 .text._reinit_peripheral_if_needed
                0x00000000000052ac       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
                0x00000000000052ac                _reinit_peripheral_if_needed
 .text.yield    0x00000000000052cc        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
                0x00000000000052cc                yield
 .text.pinMode  0x00000000000052d4       0x54 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
                0x00000000000052d4                pinMode
 .text.digitalWrite
                0x0000000000005328       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
                0x0000000000005328                digitalWrite
 .text.millis   0x0000000000005340       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
                0x0000000000005340                millis
 .text._GLOBAL__sub_I__reinit_peripheral_if_needed
                0x0000000000005358       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .text.z_impl_uart_irq_tx_enable
                0x0000000000005380        0xa /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .text._ZN7arduino12ZephyrSerial5beginEm
                0x000000000000538a        0xa /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x000000000000538a                arduino::ZephyrSerial::begin(unsigned long)
 .text._ZN7arduino12ZephyrSerial3endEv
                0x0000000000005394        0xa /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000005394                arduino::ZephyrSerial::end()
 .text._ZN7arduino12ZephyrSerial5writeEh
                0x000000000000539e       0x18 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x000000000000539e                arduino::ZephyrSerial::write(unsigned char)
 .text._ZN7arduino12ZephyrSerialcvbEv
                0x00000000000053b6        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x00000000000053b6                arduino::ZephyrSerial::operator bool()
 .text._ZN7arduino12ZephyrSerial17_reinit_if_neededEv
                0x00000000000053ba        0x6 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x00000000000053ba                arduino::ZephyrSerial::_reinit_if_needed()
 .text.k_sem_give
                0x00000000000053c0        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .text.k_sem_take.isra.0
                0x00000000000053c8        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .text._ZN7arduino12ZephyrSerial4readEv
                0x00000000000053d0       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x00000000000053d0                arduino::ZephyrSerial::read()
 .text._ZN7arduino12ZephyrSerial4peekEv
                0x0000000000005418       0x48 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000005418                arduino::ZephyrSerial::peek()
 .text._ZN7arduino12ZephyrSerial17availableForWriteEv
                0x0000000000005460       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000005460                arduino::ZephyrSerial::availableForWrite()
 .text._ZN7arduino12ZephyrSerial9availableEv
                0x0000000000005494       0x34 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000005494                arduino::ZephyrSerial::available()
 .text._ZN7arduino12ZephyrSerial5beginEmt
                0x00000000000054c8       0xc0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x00000000000054c8                arduino::ZephyrSerial::begin(unsigned long, unsigned short)
 .text._ZN7arduino12ZephyrSerial5flushEv
                0x0000000000005588       0x2c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000005588                arduino::ZephyrSerial::flush()
 .text._ZN7arduino12ZephyrSerial5writeEPKhj
                0x00000000000055b4       0x70 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x00000000000055b4                arduino::ZephyrSerial::write(unsigned char const*, unsigned int)
 .text._ZN7arduino12ZephyrSerial10IrqHandlerEv
                0x0000000000005624       0xec /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000005624                arduino::ZephyrSerial::IrqHandler()
 .text._ZN7arduino12ZephyrSerial11IrqDispatchEPK6devicePv
                0x0000000000005710        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000005710                arduino::ZephyrSerial::IrqDispatch(device const*, void*)
 .text._ZN7arduino12ZephyrSerial18ZephyrSerialBufferILi64EEC2Ev
                0x000000000000571c       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x000000000000571c                arduino::ZephyrSerial::ZephyrSerialBuffer<64>::ZephyrSerialBuffer()
                0x000000000000571c                arduino::ZephyrSerial::ZephyrSerialBuffer<64>::ZephyrSerialBuffer()
 .text._GLOBAL__sub_I__ZN7arduino12ZephyrSerial5beginEmt
                0x0000000000005744       0x5c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .text.unlikely._ZSt17__throw_bad_allocv
                0x00000000000057a0        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
                0x00000000000057a0                std::__throw_bad_alloc()
 .text.unlikely._ZSt20__throw_length_errorPKc
                0x00000000000057a6        0x6 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
                0x00000000000057a6                std::__throw_length_error(char const*)
 *(.text.*)
 *(.text._*)
 *(.init)
 *(.ctors)
 *(.dtors)
 *(.fini)

.static_thread_data_area
                0x00000000000057ac        0x0
                0x00000000000057ac                __static_thread_data_list_start = .
 *(.static_thread_data_area SORT_BY_NAME(.__static_thread_data.*))
                0x00000000000057ac                __static_thread_data_list_end = .

.data
 *(.data .data.*)

.bss            0x00000000000057b0     0x18c8
 *(.bss .bss.* COMMON)
 .bss._ZGVN12RouterBridge3HCIE
                0x00000000000057b0        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000057b0                guard variable for RouterBridge::HCI
 .bss._ZGVZN7arduino7msgpack8Unpacker10from_arrayIJRiRNS_6StringEEEEbDpOT_E2sz
                0x00000000000057b4        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000057b4                guard variable for arduino::msgpack::Unpacker::from_array<int&, arduino::String&>(int&, arduino::String&)::sz
 .bss._ZZN7arduino7msgpack8Unpacker10from_arrayIJRiRNS_6StringEEEEbDpOT_E2sz
                0x00000000000057b8        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000057b8                arduino::msgpack::Unpacker::from_array<int&, arduino::String&>(int&, arduino::String&)::sz
 .bss._ZN12RouterBridge3HCIE
                0x00000000000057bc       0x28 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000057bc                RouterBridge::HCI
 .bss._ZGVZN17RpcDecoderManager11getInstanceEvE8instance
                0x00000000000057e4        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000057e4                guard variable for RpcDecoderManager::getInstance()::instance
 .bss._ZZN17RpcDecoderManager11getInstanceEvE8instance
                0x00000000000057e8       0x1c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x00000000000057e8                RpcDecoderManager::getInstance()::instance
 *fill*         0x0000000000005804        0x4 
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE1t
                0x0000000000005808       0x10 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005808                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::t
 .bss._ZGVZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE1e
                0x0000000000005818        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005818                guard variable for RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::e
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE1e
                0x000000000000581c        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000581c                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::e
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE6map_sz
                0x0000000000005828        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005828                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::map_sz
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE6arr_sz
                0x000000000000582c        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000582c                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::arr_sz
 .bss._ZGVZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE5bytes
                0x0000000000005830        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005830                guard variable for RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::bytes
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE5bytes
                0x0000000000005834        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005834                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::bytes
 .bss._ZGVZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE6string
                0x0000000000005840        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005840                guard variable for RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::string
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE6string
                0x0000000000005844        0xc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005844                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::string
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE5num64
                0x0000000000005850        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005850                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::num64
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE5num32
                0x0000000000005858        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005858                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::num32
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE7integer
                0x000000000000585c        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x000000000000585c                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::integer
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE1b
                0x0000000000005860        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005860                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::b
 .bss._ZZN8RpcUtils6detail12unpackObjectERN7arduino7msgpack8UnpackerEE3nil
                0x0000000000005861        0x1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
                0x0000000000005861                RpcUtils::detail::unpackObject(arduino::msgpack::Unpacker&)::nil
 *fill*         0x0000000000005862        0x2 
 .bss.Monitor   0x0000000000005864      0x238 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000005864                Serial
                0x0000000000005864                Monitor
 *fill*         0x0000000000005a9c        0x4 
 .bss.Bridge    0x0000000000005aa0      0x168 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
                0x0000000000005aa0                Bridge
 .bss._ZL18arduino_pin_timers
                0x0000000000005c08     0x1180 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .bss._ZL12pinmux_array
                0x0000000000006d88      0x118 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .bss.Serial2   0x0000000000006ea0       0xec /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000006ea0                Serial2
 .bss.Serial1   0x0000000000006f8c       0xec /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
                0x0000000000006f8c                Serial1
 *(.noinit .noinit.*)

.exported_sym   0x0000000000007078        0x8
 *(.exported_sym)
 .exported_sym  0x0000000000007078        0x8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 *(.exported_sym.*)

.init_array     0x0000000000007080       0x10
 *(.init_array)
 .init_array    0x0000000000007080        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .init_array    0x0000000000007084        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .init_array    0x0000000000007088        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .init_array    0x000000000000708c        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)

.fini_array     0x0000000000007090        0x8
 *(.fini_array)
 .fini_array    0x0000000000007090        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .fini_array    0x0000000000007094        0x4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o

.symtab
 *(.symtab)

.strtab
 *(.strtab)

.shstrtab
 *(.shstrtab)

.got
 *(.got .got.* .got.plt .got.plt*)
OUTPUT(/home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch.ino_debug.elf elf32-littlearm)
LOAD linker stubs

.debug_info     0x0000000000000000    0x706db
 .debug_info    0x0000000000000000    0x2bcbf /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .debug_info    0x000000000002bcbf    0x2be0b /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .debug_info    0x0000000000057aca     0x2d13 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .debug_info    0x000000000005a7dd     0x1f74 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .debug_info    0x000000000005c751     0x3e0c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .debug_info    0x000000000006055d     0x1d6b /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .debug_info    0x00000000000622c8     0x1e2b /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .debug_info    0x00000000000640f3      0x7af /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .debug_info    0x00000000000648a2     0x1f7a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .debug_info    0x000000000006681c     0x651c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .debug_info    0x000000000006cd38     0x39a3 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)

.debug_abbrev   0x0000000000000000     0x5b03
 .debug_abbrev  0x0000000000000000     0x1403 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .debug_abbrev  0x0000000000001403     0x1380 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .debug_abbrev  0x0000000000002783      0x594 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .debug_abbrev  0x0000000000002d17      0x500 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .debug_abbrev  0x0000000000003217      0x5d4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .debug_abbrev  0x00000000000037eb      0x1e9 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .debug_abbrev  0x00000000000039d4      0x538 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .debug_abbrev  0x0000000000003f0c      0x234 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .debug_abbrev  0x0000000000004140      0x4d6 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .debug_abbrev  0x0000000000004616      0xba6 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .debug_abbrev  0x00000000000051bc      0x947 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)

.debug_loclists
                0x0000000000000000    0x18671
 .debug_loclists
                0x0000000000000000     0x913d /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .debug_loclists
                0x000000000000913d     0x941c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .debug_loclists
                0x0000000000012559     0x12da /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .debug_loclists
                0x0000000000013833      0x883 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .debug_loclists
                0x00000000000140b6     0x1943 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .debug_loclists
                0x00000000000159f9      0xb87 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .debug_loclists
                0x0000000000016580       0x72 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .debug_loclists
                0x00000000000165f2      0x2bc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .debug_loclists
                0x00000000000168ae       0xd1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .debug_loclists
                0x000000000001697f     0x153b /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .debug_loclists
                0x0000000000017eba      0x7b7 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)

.debug_aranges  0x0000000000000000     0x1270
 .debug_aranges
                0x0000000000000000      0x468 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .debug_aranges
                0x0000000000000468      0x410 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .debug_aranges
                0x0000000000000878      0x128 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .debug_aranges
                0x00000000000009a0       0x90 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .debug_aranges
                0x0000000000000a30      0x298 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .debug_aranges
                0x0000000000000cc8      0x280 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .debug_aranges
                0x0000000000000f48       0x38 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .debug_aranges
                0x0000000000000f80       0xb0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .debug_aranges
                0x0000000000001030       0x20 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .debug_aranges
                0x0000000000001050      0x158 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .debug_aranges
                0x00000000000011a8       0xc8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)

.debug_rnglists
                0x0000000000000000     0x36f4
 .debug_rnglists
                0x0000000000000000     0x14c2 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .debug_rnglists
                0x00000000000014c2     0x1460 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .debug_rnglists
                0x0000000000002922      0x1c1 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .debug_rnglists
                0x0000000000002ae3      0x103 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .debug_rnglists
                0x0000000000002be6      0x375 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .debug_rnglists
                0x0000000000002f5b      0x1db /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .debug_rnglists
                0x0000000000003136       0x33 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .debug_rnglists
                0x0000000000003169       0x7f /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .debug_rnglists
                0x00000000000031e8       0x46 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .debug_rnglists
                0x000000000000322e      0x2fe /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .debug_rnglists
                0x000000000000352c      0x1c8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)

.debug_line     0x0000000000000000    0x1732b
 .debug_line    0x0000000000000000     0x7d11 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .debug_line    0x0000000000007d11     0x7816 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .debug_line    0x000000000000f527      0xc5a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .debug_line    0x0000000000010181      0x8d4 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .debug_line    0x0000000000010a55     0x1a12 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .debug_line    0x0000000000012467      0x77b /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .debug_line    0x0000000000012be2      0x839 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .debug_line    0x000000000001341b      0x36b /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .debug_line    0x0000000000013786      0x870 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .debug_line    0x0000000000013ff6     0x237d /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .debug_line    0x0000000000016373      0xfb8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)

.debug_str      0x0000000000000000    0x4a3b8
 .debug_str     0x0000000000000000    0x1d825 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .debug_str     0x000000000001d825    0x1dd7a /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .debug_str     0x000000000003b59f     0x16d0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .debug_str     0x000000000003cc6f     0x167e /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .debug_str     0x000000000003e2ed     0x1828 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .debug_str     0x000000000003fb15      0x886 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .debug_str     0x000000000004039b     0x1fdf /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .debug_str     0x000000000004237a      0x4d7 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .debug_str     0x0000000000042851     0x1c17 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .debug_str     0x0000000000044468     0x3484 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .debug_str     0x00000000000478ec     0x2acc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)

.debug_frame    0x0000000000000000     0x3dc0
 .debug_frame   0x0000000000000000     0x1168 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/sketch/sketch.ino.cpp.o
 .debug_frame   0x0000000000001168      0xfac /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/libraries/Arduino_RouterBridge/singletons.cpp.o
 .debug_frame   0x0000000000002114      0x3d0 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Print.cpp.o)
 .debug_frame   0x00000000000024e4      0x1fc /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(Stream.cpp.o)
 .debug_frame   0x00000000000026e0      0x7e8 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(String.cpp.o)
 .debug_frame   0x0000000000002ec8      0x510 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(llext_wrappers.c.o)
 .debug_frame   0x00000000000033d8       0x68 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(main.cpp.o)
 .debug_frame   0x0000000000003440      0x140 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(new.cpp.o)
 .debug_frame   0x0000000000003580       0x40 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(threads.cpp.o)
 .debug_frame   0x00000000000035c0      0x45c /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrCommon.cpp.o)
 .debug_frame   0x0000000000003a1c      0x220 /home/arduino/ArduinoApps/demo_10_stepper_motor/.cache/sketch/core/core.a(zephyrSerial.cpp.o)
 .debug_frame   0x0000000000003c3c      0x184 /home/arduino/.arduino15/packages/zephyr/tools/arm-zephyr-eabi/0.16.8/bin/../lib/gcc/arm-zephyr-eabi/12.2.0/../../../../arm-zephyr-eabi/lib/thumb/v8-m.main+fp/hard/libstdc++_nano.a(functexcept.o)
